| Responding CAN ID | Frame (Hex) | Description | Expected Decoded Value |

|-------------------|------------------|--------------------------------------------------|---------------------------------|

| 0x500 | 03 | Speed = 100, RPM = 120 → Status = 3 | fuelEconomyStatus = 3 |

| 0x500 | 02 | Speed = 80, RPM = 90 → Status = 2 | fuelEconomyStatus = 2 |

| 0x500 | 01 | Speed = 50, RPM = 60 → Status = 1 | fuelEconomyStatus = 1 |

| 0x500 | 00 | Speed = 20, RPM = 30 → Status = 0 | fuelEconomyStatus = 0 |

| 0x600 | 02 | Pressure = 15, Level = 25, Temp = 65 → Status = 2| fuelStatusCode = 2 |

| 0x600 | 01 | Pressure = 25, Level = 35, Temp = 55 → Status = 1| fuelStatusCode = 1 |

| 0x600 | 00 | Pressure = 30, Level = 50, Temp = 45 → Status = 0| fuelStatusCode = 0 |

| 0x610 | 03 00 00 00 | Current = 5, Health = 0, Temp = 65 → Status = 3 | batteryStatusCode = 3 |

| 0x610 | 02 00 00 00 | Current = 15, Health = 0, Temp = 55 → Status = 2 | batteryStatusCode = 2 |

| 0x610 | 01 00 00 00 | Current = 15, Health = 1, Temp = 55 → Status = 1 | batteryStatusCode = 1 |

| 0x610 | 00 00 00 00 | Current = 15, Health = 1, Temp = 45 → Status = 0 | batteryStatusCode = 0 |

| 0x620 | 02 00 00 00 | GPS Accuracy = 25, Status = 1 → Status = 2 | navigationStatusCode = 2 |

| 0x620 | 01 00 00 00 | GPS Accuracy = 35, Status = 1 → Status = 1 | navigationStatusCode = 1 |

| 0x620 | 00 00 00 00 | GPS Accuracy = 40, Status = 2 → Status = 0 | navigationStatusCode = 0 |

| 0x630 | 02 00 00 00 | Cabin Temp = 36, Air Quality = 0 → Status = 2 | climateControlStatusCode = 2 |

| 0x630 | 01 00 00 00 | Cabin Temp = 30, Air Quality = 1 → Status = 1 | climateControlStatusCode = 1 |

| 0x630 | 00 00 00 00 | Cabin Temp = 25, Air Quality = 1 → Status = 0 | climateControlStatusCode = 0 |

| 0x640 | 02 00 00 00 | Front Left = 28 → Status = 2 | tireStatusCode = 2 |

| 0x640 | 02 00 00 00 | Rear Right = 25 → Status = 2 | tireStatusCode = 2 |

| 0x640 | 02 00 00 00 | Rear Left = 29 → Status = 2 | tireStatusCode = 2 |

| 0x640 | 02 00 00 00 | Front Right = 20 → Status = 2 | tireStatusCode = 2 |

| (none) | (none) | All pressures ≥ 30 → No status sent | (No frame transmitted) |